
Parameters for C:\MassLynx\Projects\CSF_MTG.PRO\ACQUDB\NT.EXP

Data Processing:
SIR / MRM Chromatogram Spike Removal	ON
SIR / MRM Smoothing		OFF
Smoothing window size (scans)	3
Number of smooths		2


Prescan Statistics:
Initial Average Intensity	3727.0291
Initial Average Std Dev		2.0829
Bunch Zero Level		0.0155
Bunch Std Dev			0.6198
Bunch Threshold			4.9584


Method Events:
Initial Stop Flow:	No Change
Initial Switch 2:	No Change
Initial Switch 3:	No Change
Initial Switch 4:	No Change
Initial Infusion:	No Change
Initial Flow State:	LC
Initial Flow Rate:	5
Initial Reservoir:	No Action
API Probe Delay Temp:	20
Initial Refill:		No Action
Timed Events Enabled
Event	Time(Sec)	Name		Action
1	0.00		Flow State	Waste
2	30.00		Flow State	LC
3	240.00		Flow State	Waste


Source Information:
Type - ESI
Status - Option Connector Disconnected

Ion Count Threshold:	350.0000

Instrument Parameters - Function 1:
Parameter File - C:\MassLynx\Projects\CSF_MTG.PRO\ACQUDB\Default.ipr
Polarity	ES+
Calibration	Static 2
Capillary (kV)	2.50
Cone (V)	30.00
Source Temperature (°C)	150
Desolvation Temperature (°C)	450
Cone Gas Flow (L/Hr)	50
Desolvation Gas Flow (L/Hr)	900
Collision Gas Flow (mL/Min)	ON
LM 1 Resolution	4.30
HM 1 Resolution	14.80
Ion Energy 1	-0.60
MS Mode Collision Energy	3.00
MS Mode Entrance (Gas On)	1.00
MS Mode Exit (Gas On)	1.00
MS Mode Entrance (Gas Off)	1.00
MS Mode Exit (Gas Off)	1.00
MSMS Mode Collision Energy	20.00
MSMS Mode Entrance (Gas On)	1.00
MSMS Mode Exit (Gas On)	1.00
MSMS Mode Entrance (Gas Off)	1.00
MSMS Mode Exit (Gas Off	1.00
LM 2 Resolution	10.60
HM 2 Resolution	14.10
Ion Energy 2	0.30
Gas On MS Mode Entrance	1.00
Gas On MS Mode Exit	1.00
Gas On MSMS Mode Entrance	1.00
Gas On MSMS Mode Exit	1.00
Gas Off MS Mode Entrance	1.00
Gas Off MS Mode Exit	1.00
Gas Off MSMS Mode Entrance	1.00
Gas Off MSMS Mode Exit	1.00
Gain	1.00
Active Reservoir	A
Cone Voltage Ramp :Disabled
Probe Temperature Ramp :Disabled


Engineers Settings:
MS1 Low Mass Position      	519
MS1 High Mass Position     	225
MS1 Low Mass Resolution    	511
MS1 High Mass Resolution   	1950
MS1 Resolution Linearity   	888
MS1 High Mass DC Balance   	-0.35
MS1 DC Polarity            	Positive
MS2 Low Mass Position      	520
MS2 High Mass Position     	197
MS2 Low Mass Resolution    	512
MS2 High Mass Resolution   	1343
MS2 Resolution Linearity   	852
MS2 High Mass DC Balance   	-0.45
MS2 DC Polarity            	Negative
HM RF Lens Correction + 	0.00
HM RF Lens Correction - 	0.00


   Instrument Readbacks   
Capillary (kV)	2.50
Cone (V)	17.83
Extractor (V)	0.00
Source Temperature (°C)	148
Desolvation Temperature (°C)	449
Cone Gas Flow (L/Hr)	50
Desolvation Gas Flow (L/Hr)	894
Collision Gas Flow (mL/Min)	ON


Inter-scan delays:
Automatic Mode - See Help Files for details
